|  |  |  |  |
| --- | --- | --- | --- |
| **Body Pro-Lok ONE™ System**  **with ONEPlatform™ or Universal Couchtop™** | |  | |
| Patient |  | Date |  |
| Notes |  | | |

**IMPORTANT INSTRUCTIONS, PLEASE READ:**When indexing to the Universal Couchtop, use the indexing marks along the side of the couchtop for indexing Lok-Bars™ and the indexing marks along the top of the couchtop for indexing Body Pro-Lok ONE devices.

* When transferring a setup from the Universal Couchtop or ONEPlatform to the Body Pro-Lok ONE Rails-Only System, the ONEBridge™ must be adjusted and set 50 mm lower than on the Universal Couchtop or ONEPlatform\*.
* When transferring a setup from the Universal Couchtop or ONEPlatform to the iBEAM® evo Couchtop with the Body Pro-Lok ONE evo Adapter, reference Appendix A for available setup regions\*.

*\*Separate set-up sheets for Body Pro-Lok ONE Rails-Only and evo Adapter are available.*

**If utilizing the ONEPlatform, start at #1  
If indexing directly to the Universal Couchtop, start at “Respiratory Plate” (page 2)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Lok-Bars for indexing the ONEPlatform are indexed to table at | | |  | |
| Lateral Lok-Bar Position | F  G  H | | | |
| Lateral Position (only if using a Transverse Lok-Bar) | | | | |
| Head end indexed at: |  | Foot End Indexed at: | |  |
|  | |  | | |

|  |  |  |
| --- | --- | --- |
| Respiratory Plate Used | Standard  Wide  ComfortCare™ Cushion | |
| 1) ONEBridge Side A |  |  |
| 2) ONEBridge Side B |  |
| 3) Docking Index |  |
| 4) ONEBridge Lateral Position |  |
| 5) Respiratory Plate Height |  |
| 6) Respiratory Plate   Lateral Position | D  C  E |
| **If using ComfortCare Cushion with  Wide Respiratory Plate)**  7) Set pressure between | & |  |

|  |  |  |
| --- | --- | --- |
| Respiratory Belt Used? | Yes   No |  |
| 1) Docking Index |  |
| 2) Left velcro strap indexed at |  |
| 3) Right velcro strap indexed at |  |
| 4) Set pressure between | & |

|  |  |  |  |
| --- | --- | --- | --- |
| Patient hAND GRIPS USED? | Yes  No | | |
| rIGHT HAND GRIP INDEXED AT |  | lEFT HAND GRIP INDEXED AT |  |

|  |  |  |
| --- | --- | --- |
| Bridge with Clam-Lok  Cushion Used? | Yes   No | Diagram, engineering drawing  Description automatically generated |
| 1) ONEBridge Side A |  |
| 2) ONEBridge Side B |  |
| 3) Docking Index |  |
| 4) ONEBridge Lateral Position |  |

|  |  |  |  |
| --- | --- | --- | --- |
| KneeFix Used? | Yes  No | Indexed To  PLATFORM AT |  |
| Feetfix Used? | Yes  No | Indexed To  PLATFORM AT |  |
| flexlock knee support used? | High  Low | Indexed To  PLATFORM AT |  |
| location of knee support on Locating Bar | A B C D  E V W X  Y Z |
| Flexlock feet support used? | Yes  No | Indexed To  PLATFORM AT |  |
| location of feet support on locating bar | A B C  D E |
| Angle of Feet Support | 0° 5° 10°  15° 20° 25°  30° |
| leg and Foot Strap used? | Yes  No |
| Additional indexable accessory |  | Indexed To  PLATFORM AT |  |
| Additional indexable accessory |  | Indexed To  PLATFORM AT |  |